#000000
#082C60
#67201B
#521F1D
#B92A25
#204B5C
#1F4564
#6C393C
#1588BD
#5E471E
#BA5C23
#766330
#454722
#46573A
#9F6830
#637A3F
#9E852B
#999F3B
#832920
#7E501D
#604F2A
#67592E
#562819
#484231
#27383C
#AF4C36
#526958
#E59C1C
#C68542
#A59045
#7B5339
#C69E67
#F8DC18
#CBC029

🎨 Color Limitations in Underglaze Serigraphy Printing

In serigraphy printing with underglaze paints, the available color palette is limited. Notably, white is not included among underglaze colors, which restricts the ability to create tonal variations. The hex codes listed above represent the full range of usable colors.

To achieve certain tones, we layer multiple colors during printing. This method allows us to approximate the desired hues within the constraints of the underglaze system.

All pattern design and layout work is carried out using CorelDraw 2022, ensuring precision and compatibility with the serigraphy process.